NTC thermistor.

Use the dial to adjust temperature.

Property: (default value)

Main:
- Minimum Value: (0 ºC)
   Temperature with dial at the left end.

- Maximum Value: (200 ºC)
   Temperature with dial at the right end.

- Current Value: (25 ºC)
   Value determined by dial position.

- Dial Step: (0 ºC)
   Minimum step when rotating the dial.
   0 to use default.


Parameters:
- B: (3455)
   β parameter.

- R25: (10000 Ω)
   Resistance at 25 ºC.

#include dialed
