Resistive touchpad.

Property: (default value)

Main:
- Width (240 pixels)

- Height: (320 pixels)

- Transparent (no)

Electric:
- RxMin: (100 Ω)
   Minimum resistance in X axis (right side).

- RxMax: (100 Ω)
   Maximum resistance in X axis (left side).

- RyMin: (100 Ω)
   Minimum resistance in Y axis (top side).

- RyMax: (100 Ω)
   Maximum resistance in Y axis (bottom side).
