
**1.Features:**

* Contact form: 1a, 1b, 1c
* Rated load: 10A 250VAC/28VDC,10A 125VAC/28VDC,10A 125VAC/28VDC
* Contact resistance: <=100m (ohm)
* Electrical life: 100,000
* Mechanical life: 10,000,000

**2.Parameters:**

* Coil rated voltage: 3-48VDC
* Coil power: 0.36W, 0.45W
* Coil pick-up voltage: <=75%
* Coil drop-out voltage: >=10%
* Ambient temperature: -25 degrees Celsius to +70 degrees Celsius
* Coil and contacts:1500VAC/min
* Contact and contacts: 1000VAC/min
* Insulation resistance: >=100M (ohm)



Reference circuit

