Sezioni di filettatura standard

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | **Raccordo** | **Ø (mm)** | **L (mm)** |
| **Raccordo tubo** Attacco standard per fascetta stringitubo | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-hose.jpg | 6.3 mm (1/4") 8 mm (5/16") 10 mm (3/8") 13 mm (1/2") 18 mm (5/8") | - - - - - | 18.0 18.0 21.0 21.0 21.0 |
| **Raccordo Stream-line** Attacco per tubo con tenuta conica su maschio e dado | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-stream-line.jpg | 5 x 8 mm 6.5 x 10 mm 8 x 12 mm 9.5 x 13.5 mm 11 x 16 mm | - - - - - | 15.0 17.0 19.0 21.0 25.0 |
| **Raccordo CEJN-lock** Per tubo senza graffatura o fascette | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-cejn-lock.jpg | 1/4" 3/8" 1/2" | - - - | 19.0 23.0 26.0 |
| **Filettatura UNF** Filettatura unificata conforme ISO 68, ANSI B1.1  Maschio: es. 9/16"-18 UNF  Femmina: es. 7/16"-20 UNF  Femmina, SEA O-Ring Boss | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-unf-male.jpg https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-unf-female_2.jpg | **Male Thread** 7/16"-20 UNF 7/8"-14 UNF    **Filettatura femmina** 7/16"-20 UNF 9/16"-18 UNF 3/4"-16 UNF 1 1/16"-16 UNF 1 5/16"-12 UNF | 11.0 22.0     9.8 12.9 17.5 26.8 33.1 | 13.3 15.5     11.5 12.7 14.3 19.0 19.0 |
| **Filettatura Metrica** Filettatura metrica conforme ISO 68 / ISO 724  Maschio: es. M16x1.5  Femmina: es. M16x1.5 | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-metric-male.jpg https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-unf-female_2.jpg | **Male Thread** M10x1.25 M12x1.5 M14x1.5 M16x1.5 M22x1.5  **Filettatura femmina** M16x1.5 | 9.8 11.85 13.85 15.85 21.85   14.5 | 9.0 13.0 13.0 8.81 15.7   9.0 |
| **Raccordo filettato R/Rc** Filettatura conica conforme ISO 7/1  (altre descrizioni comuni sono BSPT, Kr)   Maschio: es. R 1/4"  Femmina: es. Rp 1/4" (cilidrica) es. Rc 1/4" (conica) | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-r-male.jpg https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-rc-female.jpg | **Male Thread** R 1/8" R 1/4" R 3/8" R 1/2" R 3/4"  **Filettatura femmina** Rc 1/8" Rc 1/4" Rc 3/8" Rc 1/2" Rc 3/4" | 10.2 13.6 17.2 21.7 27.1   8.3 11.0 14.5 18.0 23.5 | 7.4 11.0 11.0 15.0 16.3   7.4 11.0 11.4 15.0 16.3 |
| **Raccordo filettato G** Filettatura cilindrica conforme ISO 228/1  (altre descrizioni comuni sono BSP, R)  Maschio: es. G 1/4"   Femmina (ISO 1179): es. G 1/4" | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-g-male_2.jpg https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-unf-female_2.jpg | **Male Thread** G 1/8" G 1/4" G 3/8" G 1/2" G 3/4"  **Filettatura femmina** G 1/8" G 1/4" G 3/8" G 1/2" G 3/4" | 9.6 13.0 16.5 20.8 26.3   8.75 11.8 15.25 19.0 24.5 | 8.0 10.0 10.0 12.0 12.0   7.4 11.0 11.4 15.0 16.3 |
| **Raccordo filettato NPT** Filettatura standard americana conforme ANSI/ASME B 1.20.1  Maschio e Femmina: es. 1/4" NPT | https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-npt-male.jpg https://cdn.cejn.com/globalassets/images/global-guides--support/thread-standards/connection-npt-female.jpg | **Male Thread** 1/8" NPT 1/4" NPT 3/8" NPT 1/2" NPT 3/4" NPT  **Filettatura femmina** 1/8" NPT 1/4" NPT 3/8" NPT 1/2" NPT 3/4" NPT | 10.5 14.0 17.5 21.8 27.1   8.5 11.0 14.5 18.0 23.0 | 6.7 10.2 10.4 13.6 13.9   6.9 10.0 10.3 13.6 14.1 |