Force Sensor.

Use the dial to adjust force.

Property: (default value)

Main:
- Minimum Value: (0 N)
   Force in Newtons with dial at the left end.

- Maximum Value: (1000 N)
   Force in Newtons with dial at the right end.

- Current Value: (0 N)
   Value determined by dial position.

- Dial Step: (0 N)
   Minimum step when rotating the dial.
   0 to use default.


Parameters:
- Ref. Temperature: (20 ºC)
   Reference Temperature.

- Temperature: (20 ºC)
   Current Temperature.

#include dialed
